Specification for Sports Utility Vehicle
Chassis:  type 4 X 4  4WD, Year: 2003 – 2004

Engine type: Petrol 6 cylinder in line 4 strokes Water cooled tropical

Engine power:  220 hp or greater, Clutch/hydraulic operated dray single plate
Gear box: Manual, 4 door plus rear hutch back rear door 

7 Passenger,  

Power steering / left hand drive

Power windows, central locking

Air conditioner, heater and defroster
AM/FM RADIO CASSETTE

AIR CONDITION AND HEATING SYSTEM AND DEFROSTER 

THE CAN MUST MEET ISO 9001

DIGITAL QUARTZ CLOCK 

HOLOGEN HEAD LAMPS

EQUIPPED WITH 

SPARE TIRE 

LIFTING JACK 

FIRE EXTINGUISHER 

TOOLS (contractor must included list of tools in proposal)
SPARE PARTS FOR 2 YEARS (a list of spare parts that vendors intend to provided must be included in the technical proposal)
MAINENANCE FOR 12 MONTHS (maintenance plan must be included in technical proposal)

1 year warranty against mechanical failure and manufacture defected 
