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                 Genuine replacement parts: NO SUBSTITUTIONS
	ITEM
	DESCRIPTION
	QUANTITY
	UNIT

	001
	Seal Oil Pumps, Manufactured by Weir Pump LTD (England)

-Type-  IMO Screw type
-Capacity - 540 L/min
-Suction = Flooded
-Discharge Pressure - 10 BAR
-Liquid temperature -25 to 56 C
-Serial No. 62711-00118
-Vertical K Type 
 
	4
	EA

	002
	Crude Oil Burner Pump, Positive Displacement Screw Type Pump, Manufacturer Weir Pumps LTD, 

-IMO Screw Type
-Frame size APG 110-8BN3EH
-Weir Serial No. 62797-030/41
-Liquid temperature, 50 to 0 C
-Viscosity, 2-220 cst
-Capacity 54-73 m3/hr
-Suction Lift  5 M
-Discharge pressure,  41 kg/cm2
-Relief valve setting  46 kg/cm2 
 
	4
	EA

	003
	
Heavy Oil Burner Pump, Positive displacement screw pump, Manufacturer Weir Pumps LTD, - IMO screw type -Frame size ALG 90-4N3EH -Weir Serial No. 62797-006/17 -Arrangement - Horizontal -Liquid temperature 115 - 50 C -Specific Gravity 0.95 -Viscosity 240 -1200 cst -Capacity 51.7 - 54.6 m3/hr -Suction lift 5 M -Discharge pressure 44 kg/cm2 -Relief valve setting 45 kg/cm2 Note: Provide three pumps with motor as listed in item 4. 


	4
	EA

	004
	Boiler Heavy Oil Burner Motor, 110 kW, 380 V, 50 Hz, 3-phase, 1450 rpm, Frame Size: E3 15 S. Type: Squirrel Cage. Enclosure: TEFC, IP55, EXD. Insulation Class: F. Manufacturer: GEC Machines Limited


	3
	EA

	005
	Flexible Coupling, for coupling Boiler Heavy Oil Burner Pump with motor
	3
	EA
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