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 Specifications 

Night Vision Devices
The contractor/vendor shall prepare and submit a proposal in accordance with the following specifications.


Individual Night Vision Device: This individual system will allow squad leaders, patrol leaders, and above to have night vision capability.    Salient features are:
· Allow users to engage targets in low light levels with AK-47 and RPK light machine gun.

· Can be mounted to an individuals head with adjustable straps.

·  Must have Helmet Mounting Kit

· Allow individuals to drive vehicles and conduct low light level operations with all items and equipment identified in this statement of work.

· Allow operations in low light level conditions.  Low light level is considered to evening (Sunset to Sunrise) hours with 10% or greater moonlight illumination.
· Be battery operated with an individual battery life of eight hours of continuous operations without degradation.

· Delivered with either 25 batteries per the quantity identified in schedule B or 6 sets of rechargeable batteries and 1 recharger per the quantity identified in schedule B.
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END SPECIFICATION

