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 Binoculars:  Must have a mil reticule pattern. This will be a 10x50 or 7x50 ruggedized binocular to provide short range observation for leaders within the battalion.  It must be subdued in color.
Compass:  Must be capable of measuring accurate bearings in mils and degrees.  This will be a ruggedized magnetic compass to allow for azimuth determination and land navigation assistance.  It must be subdued in color.
GPS: This will be a ruggedized, but non-developmental, commercially available Global Positioning System.  It must use commercially available batteries. Must be base line model.
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END SPECIFICATION

