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Attachment 1 – Reference No. W914NS-04-RFI-2364 - Electrical Work Instruments

Commercial Items for Iraqi Reconstruction

	0001
	HIGH VACUUM OIL PURIFIER (3,500 L/HR) – Specially developed for the treatment of transformer insulating oil by the combined action of filtration and evaporation in a high vacuum environment.  Semi-mobile trailer complete with spare parts for fine filter cartridges.  Suggested brand name type or like type/model:  None.
	14
	ea

	0002
	HIGH VACUUM OIL PURIFIER (2,500 L/HR) – Specially developed for the treatment of transformer insulating oil by the combined action of filtration and evaporation in a high vacuum environment.  Semi-mobile trailer complete with spare parts for fine filter cartridges.  Suggested brand name type or like type/model:  None.
	14
	ea

	0003
	PRIMARY CURRENT INJECTION SET – Portable current injection set for testing primary circuit with suitable cables for high current injection.  Inlet:  2 phase, 416 Volt, 50 Hz.  Outlet:  100 – 400 – 1500 – 3000 amps.  Accessories: Cables with suitable clamps.  Suggested brand name type or like type/model:  None.
	30
	ea

	0004
	SECONDARY CURRENT INJECTION SET – Relay testing unit.  Inlet: 220 Volt, 50 Hz.  Current: 0 – 10 – 100 amps with coarse and fine adjustments.  Voltage: 0 – 250 Volt (AC/DC), Electronic timer stopped through make/break contact.  Suitable accessories.  Suggested brand name type or like type/model:  None.
	30
	ea

	0005
	INSULATION TESTER (MEGGER 5,000 VOLT) – Ranges: 5000 – 2500 – 1000 – 500 Volt.  Energized by push button and batteries.  Scale ranges: 0 – 50 Mohm, 40 – 200 Mohm, and 200 – 10000 Mohm.  Suggested brand name type or like type/model:  None.
	100
	ea

	0006
	TRANSFORMATION RATIO TESTER –   The transformer ratio shall be determined by abridge measurement, single and three phase models.  Measuring ranges: 1 – 1000 ohms.  Power source: 220 V, 50 Hz.  Suggested brand name type or like type/model:  None.
	30
	ea

	0007
	EARTH RESISTANCE METER – For measuring earth resistance and earth resistivity.  Measuring ranges 0 -9.99 kohm.  Electronic type energized by push button and batteries.  Complete accessories required.  Suggested brand name type or like type/model:  None
	30
	ea

	0008
	OIL DIELECTRIC STRENGTH TESTER – Automatic and semi-automatic voltage increase (Alternative – Programmable).  Rate of voltage rise: 0.5 – 3 kV/sec.  Supply voltage:  220 Volt, 50 Hz.  Output voltage RMS between electrodes: 10 – 70 kV.  Switching by push-buttons (Supply “ON”, and HV “ON”).  Complete accessories.  Suggested brand name type or like type/model:  None.
	30
	ea

	0009
	AVO METER – Digital multi-meter (Alternative – with temperature probe).  Current: 0 – 10 Amp (AC/DC).  Voltage: 0 – 700 Volt.  Resistance: 0 – 30 Mohm.  Suggested brand name type or like type/model:  None.
	100
	ea

	0010
	CLAMP METER – For current measurements – analogue scale (Alternative – Digital reading).  Ranges: 0 -10 – 30 – 100 – 3000 amps, 0 -700 Volt (Alternative 0 kVar, kW, Power factor.  Measuring clamp on meter.  Suggested brand name type or like type/model:  None.
	500
	ea

	0011
	HIGH TENSION AC/DC TESTER – Portable tester of output voltages continuously adjustable.  Voltage: DC – 0 – 80 kV, AC – 0- 80 kV RMS.  Supply voltage:  220 Volt, 50 Hz.  Operating unit, current limitation unit.  Accessories: Discharge rod (750 kohm connecting high voltage cable for testing.  Suggested brand name type
	100
	ea


