Communicate Via a Tactical Radio in a Secure Net

Conditions: Given an operational radio set (SINCGARS, IHFR, VRC-12 series, etc.), with an (SOI), fill device with appropriate fills, and fill cable, TM 11-5820-890-10-8, TM 11-5820-401-10-2, and an operational distant station.  
Standards: Established voice communications with the distant tactical radio/network within three minutes.

Performance Steps

1.
Place radio into operation.

a.
Preset controls.

b.
Turn radio set on.

c.
Test radio transmission (RT) circuits.

2.
Enter net.

a.
Load appropriate fills.

b.
Operate radio set.

3.
Transmit message.

a.
Establish secure communications.

b.
Use prowords, call signs, frequencies, item numbers and authentications.

Evaluation Preparation:

Setup: An operational radio set (SINCGARS, IHFR, VRC-12 series, etc.), with an (SOI), fill device with appropriate fills, and fill cable, TM 11-5820-890-10-8, TM 11-5820-401-10-2, and an operational distant station.  Brief Soldier: Tell the soldier he must establish voice communications with the distant tactical radio/network, within three minutes. The three-minute limit is only an administrative training requirement.

Performance Measures 




GO NO GO

1.
Placed radio into operation. 




—— ——

a.
Preset controls.
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b.
Turned radio set on.

c.
Tested radio transmission (RT) circuits.

2.
Entered net. 






—— ——

a.
Loaded appropriate fills.

b.
Operated radio set.

3.
Transmitted message. 





—— ——

a.
Established secure communications.

b.
Used prowords, call signs, frequencies, item numbers, and authentications.

Evaluation Guidance: Score the soldier GO if all performance measures are passed. Score the soldier NO GO if any performance measure is failed.  If the soldier fails any performance measure, show what was done wrong and how to do it correctly. Have the soldier practice until the task can be performed correctly.

References

SOI FM 24-18

TM 11-5820-401-10-2 FM 24-19
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