Communicate Via a Tactical Telephone

Conditions: Given a requirement to communicate a message via a tactical telephone and the following:

1.
An unclassified message (approximately 25 words).

2.
A tactical telephone (DNVT, TA-838/TT, TA-341()/TT, TA-1042A/U and TA-954/TT) installed in a point-to-point configuration and operating in a nonsecure mode.

Standards: Communicated the message within 10 minutes with no errors.

Performance Steps

1.
Initiate call (lift handset from cradle).

2.
Verify distant end is ready to receive message.

3.
Communicate message.

4.
Verify message is received.

5.
Disconnect call (return handset to cradle).

Evaluation Preparation:

Setup: Provide the soldier with—

1.
Tactical telephone (DNVT, TA-838/TT, TA-341()/TT, TA-1042A/U and TA-954/TT) that is installed and connected to the distant tactical telephone (DNVT, TA-838/TT, TA-341()/TT, TA-1042A/U and TA-954/TT).

2.
Tactical telephones (DNVT, TA-838/TT,TA-341()/TT, TA-1042A/U and TA-954/TT) are set to operate in the point-to-point mode.

3.
A prepared message (approximately 25 words) for the soldier to communicate.

Brief Soldier: Tell the soldier he must communicate the prepared message.

Performance Measures 




GO NO GO

1.
Initiated call (lifted handset from cradle). 


—— ——

2.
Verified distant end is ready to receive message.


—— ——

3.
Communicated message. 





—— ——

4.
Verified message was received. 




—— ——

5.
Disconnected call (returned handset to cradle). 


—— ——

Evaluation Guidance: Score the soldier GO if all performance measures are passed. Score the soldier NO GO if any performance measure is failed.  If the soldier scores NO GO, show him what was done wrong and how to do it correctly.
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